|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Current State | INPUT SYMBOL | | | | | | | | State Type  (Not Accepting or Accepting State) |
| [A-F] | x | [a-wy-zG-Z] | 0 | [1-9] | . | $ | other |
| 0 | 1 | 1 | 1 | 6 | 4 | IS | IS | IS | NOAS |
| 1 | 1 | 1 | 1 | 1 | 1 | 2 | 3 | 2 | NOAS |
| 2 | IS | IS | IS | IS | IS | IS | IS | IS | VID AVID/KW – ASWR |
| 3 | IS | IS | IS | IS | IS | IS | IS | IS | VID SVID – ASNR |
| 4 | ES | ES | ES | 4 | 4 | 7 | 5 | 5 | NOAS |
| 5 | IS | IS | IS | IS | IS | IS | IS | IS | DIL – ASWR |
| 6 | ES | 9 | ES | 5 | ES | 7 | ES | 5 | NOAS |
| 7 | 8 | 8 | 8 | 7 | 7 | 8 | 8 | 8 | NOAS |
| 8 | IS | IS | IS | IS | IS | IS | IS | IS | FPL – ASWR |
| 9 | 10 | ES | ES | 10 | 10 | ER | ER | ER | NOAS |
| 10 | 10 | ES | ES | 10 | 10 | ES | ES | 11 | NOAS |
| 11 | IS | IS | IS | IS | IS | IS | IS | IS | HIL – ASWR |
| 12 | IS | IS | IS | IS | IS | IS | IS | IS | ES – ASNR |
| 13 | IS | IS | IS | IS | IS | IS | IS | IS | ER – ASWR |

**Transition Table**